;*****************************************************************************
;
; Name:  zebrserv.inf 
;
; Function:
;	Install the Sony Ericsson Port (WDM)
;
; Copyright (c) 2007 MCCI Corporation 
;
; MCCI is a registered trademark of MCCI Corporation.
;
; NOTICE: This software is licensed, not sold.  Any modification of this
; inf file to change the reference to an operating system or to change the
; reference to a device is not permitted unless authorized in writing by
; MCCI Corporation.
;
;*****************************************************************************

[Version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Provider%
DriverVer=04/13/2007,4.40.2.1
;CatalogFile=zebrmdm.cat

;-----------------------------------------------------------------------------
; No files are copied by this file.. no filecopy init declarations are here.
;-----------------------------------------------------------------------------

;-----------------------------------------------------------------------------
; Table of Contents
;-----------------------------------------------------------------------------
[Manufacturer]
%SEMC%=SEMC

;-----------------------------------------------------------------------------
; Device-by-device entries
;-----------------------------------------------------------------------------
[SEMC]
%SerialF1%=SEMC.Install, ZEBRCR\{8272F936-117D-48be-A878-32CA24F6718D}
%SerialE1%=SEMC.Install, ZEBRCR\{8272F935-117D-48be-A878-32CA24F6718D}
%SerialD1%=SEMC.Install, ZEBRCR\{8272F934-117D-48be-A878-32CA24F6718D}
%SerialC1%=SEMC.Install, ZEBRCR\{8272F933-117D-48be-A878-32CA24F6718D}
%SerialB1%=SEMC.Install, ZEBRCR\{8272F932-117D-48be-A878-32CA24F6718D}
%SerialA1%=SEMC.Install, ZEBRCR\{8272F931-117D-48be-A878-32CA24F6718D}
%SerialG1%=SEMC.Install, ZEBRCR\{8272F937-117D-48be-A878-32CA24F6718D}
%SerialH1%=SEMC.Install, ZEBRCR\{8272F938-117D-48be-A878-32CA24F6718D}
%SerialI1%=SEMC.Install, ZEBRCR\{8272F939-117D-48be-A878-32CA24F6718D}
%SerialJ1%=SEMC.Install, ZEBRCR\{8272F930-117D-48be-A878-32CA24F6718D}
%SerialK1%=SEMC.Install, ZEBRCR\{8272F93A-117D-48be-A878-32CA24F6718D}
%SerialL1%=SEMC.Install, ZEBRCR\{8272F93B-117D-48be-A878-32CA24F6718D}


;-----------------------------------------------------------------------------
; The exclude-from-select stuff
;-----------------------------------------------------------------------------
[ControlFlags]
ExcludeFromSelect = *

;-----------------------------------------------------------------------------
; Installation instructions
;-----------------------------------------------------------------------------
[SEMC.Install]
AddReg		= SEMC.W95AddReg,SEMC.W95Overrides

;-----------------------------------------------------------------------------
;  Registry
;-----------------------------------------------------------------------------
;**** here's the stuff for W95 ports.
;**** it's in this INF file, but we'll not use it until we get enumerated.
[SEMC.W95AddReg]
HKR,,DevLoader,,*vcomm
HKR,,PortDriver,,zebrcomm.vxd
HKR,,Contention,,zebrvcd.vxd
HKR,,DCB,3,1C,00,00,00, 00,C2,01,00, 11,33,00,00, 00,00, 0a,00, 0a,00, 08, 00, 00, 11, 13, 00, 00, 00
HKR,,PortSubClass,1,01
HKR,,ConfigDialog,,serialui.dll
HKR,,EnumPropPages,,"serialui.dll,EnumPropPages"

;-----------------------------------------------------------------------------
;  Logical Configurations
;-----------------------------------------------------------------------------
[SEMC.W95Overrides]
;-- Config for 3f8 - COM1,IRQ4
HKR,Override,0000,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,03,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
10,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2f8 0 COM2 IRQ3
HKR,Override,0001,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,02,FF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
08,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 3e8 0 COM3 IRQ4
HKR,Override,0002,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,03,EF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
10,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2e8 0 COM4 IRQ3
HKR,Override,0003,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,02,EF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
08,00,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;-- Config for 3f8 - COM1 IRQAny
HKR,Override,0004,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,03,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2f8 0 COM2 IRQAny
HKR,Override,0005,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
F8,02,FF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 3e8 0 COM3 IRQAny
HKR,Override,0006,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,03,EF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for 2e8 0 COM4 IRQAny
HKR,Override,0007,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
E8,02,EF,02, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for anywhere- COMx IRQ Any
HKR,Override,0008,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
00,01,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** IRQ ***
10,00,00,00, \  ; total length of irq resource descriptor
04,00,00,00, \  ; ResType_IRQ - 0x00000004
01,00,00,00, \  ; IRQD_Flags / IRQD_Alloc_Num
FF,FF,00,00, \  ; IRQD_Req_Mask / IRQD_Reserved
\ ;*** TERMINATOR ***
00,00,00,00
;
;--- Config for anywhere- COMx IRQ None
HKR,Override,0009,1, \
00,04,00,00,00,00,00,00, \
\ ;*** I/O Range 0 ***
20,00,00,00, \  ; total length of io resource descriptor
02,00,00,00, \  ; ResType_IO = 0x00000002
01,00,0C,00, \  ; IOD_count / IOD_Type = 0x0c
00,00,00,00, \  ; IOD_Alloc_Base / IOD_Alloc_End
00,00,00,00, \  ; IOD_DesFlags / IOD_Alloc_Alias / IOD_Alloc_Decode
F8,FF,08,00, \  ; IOR_Align / IOR_nPorts
00,01,FF,03, \  ; IOR_Min / IOR_Max
00,00,00,00, \  ; IOR_RangeFlags / IOR_Alias / IOR_Decode
\ ;*** TERMINATOR ***
00,00,00,00


;-----------------------------------------------------------------------------
; STRINGS
;-----------------------------------------------------------------------------
[Strings]

;BEGIN ENG - US English Strings
Provider = "Sony Ericsson Mobile Communications AB"
SEMC = "Sony Ericsson Mobile Communications AB"


SerialA1 = "Sony Ericsson P990 Application Port"
SerialB1 = "Sony Ericsson P990 Debug Port"
SerialC1 = "Sony Ericsson M600 Application Port"
SerialD1 = "Sony Ericsson M600 Debug Port"
SerialE1 = "Sony Ericsson W950 Application Port"
SerialF1 = "Sony Ericsson W950 Debug Port"
SerialI1 = "Sony Ericsson P1 Application Port"
SerialJ1 = "Sony Ericsson P1 Debug Port"
SerialK1 = "Sony Ericsson W960 Application Port"
SerialL1 = "Sony Ericsson W960 Debug Port"

CustomerDataPath = "Sony Ericsson"
DriverSet = "Sony Ericsson Symbian 9 Drivers"
UninstallFile = "ZEBRUninstall.exe"

McciOptions = "Uninstallable NotInstallOnWinVer5"
;END ENG - US English Strings

;--- strings following this line should not be localized ---

;*** end of file ***
